**GEORGIA INSTITUTE OF TECHNOLOGY**

**ENVIRONMENTAL HEALTH AND SAFETY**

**GENERAL SAFETY**

**\_\_\_\_\_\_\_\_\_\_\_\_\_ Site Specific Plan**

This site specific plan was written by\_\_\_\_\_\_\_\_\_\_\_\_ for the \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ space.

Table of Contents

[PURPOSE 2](#_Toc111648129)

[SCOPE 2](#_Toc111648130)

[RESPONSIBILITIES 2](#_Toc111648131)

[HOURS OF OPERATION 2](#_Toc111648132)

[ACCESS TO SPACE 2](#_Toc111648133)

[MACHINE SPECIFIC ACCESS 2](#_Toc111648134)

[TRAINING REQUIREMENT 2](#_Toc111648135)

[SPACE GUIDELINES AND SAFE-WORK PRACTICES 2](#_Toc111648136)

[RECORD KEEPING 3](#_Toc111648137)

[APPENDICES 3](#_Toc111648138)

[EMERGENCY INFORMATION 3](#_Toc111648139)

[POST INJURY/ILLNESS INSTRUCTIONS 4](#_Toc111648140)

[AUTHORIZATION FORM 5](#_Toc111648141)

[MAKER SPACE/ STUDENT MACHINE SHOP USER’S AGREEMENT 7](#_Toc111648142)

[HAZARD ASSESSMENT TOOL – PPE SELECTION 8](#_Toc111648143)

[MAKER SPACE AND STUDENT MACHINE SHOP SELF-INSPECTION FORM 14](#_Toc111648144)

# PURPOSE

The purpose of this document is to provide guidance to occupants of the **\_\_\_\_\_\_\_\_\_\_\_\_\_** space to ensure a safe and productive work environment.

# SCOPE

These guidelines apply to all Georgia Tech students, staff, faculty, visitors, and occupants who actively work in this \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_space.

# RESPONSIBILITIES

This section should detail the different roles of staff/students in the space and their responsibilities.

# HOURS OF OPERATION

This section should list the respective space hours of operation and any exceptions.

# ACCESS TO SPACE

This section should list how a student/faculty/staff/visitor can receive access to the respective space.

It should detail training required, any waivers or documents that should be completed and any buddy system (if space can only be used in staff member is present) information etc.

# MACHINE SPECIFIC ACCESS

This section should detail how authorized users can get access to machines or tools in the space.

# TRAINING REQUIREMENT

This section should detail specific training requirements needed. This section can be taken out if training information is already explained in the other sections.

# SPACE GUIDELINES AND SAFE-WORK PRACTICES

This area should list all specific operating guideline and procedures that must be followed in this respective space. This section should detail PPE that must be worn in the space, what not to wear in the space, SOPS, safe equipment operation, housekeeping, areas that may be off limits without specific approval from Shop Manager, when an occupant must Stop-Work, and other safety guidelines and operational guidance for that space.

# RECORD KEEPING

This section should detail how copies of any training roster, training content and signed documents must be maintained and kept on file

# APPENDICES

## EMERGENCY INFORMATION

**Emergency Numbers**

The following list contains important emergency telephone numbers and related information.

|  |  |  |
| --- | --- | --- |
| **Type of Emergency:** | **Who to Call:** | **Phone Number and/or website:** |
| **General**  (Includes fire, police, emergency medical treatment, and off hour chemical spills) | **GTPD and EHS Emergency Phone** | **GTPD: 911** from an on-campus phone  Or  **404-894-1491** from a cell phone  **EHS Emergency Phone**: **404-216-5237** |
| **Emergency Repairs and Maintenance** | **Facilities Management**  **24- hour Trouble Call** | Area 1: **404-385-1000**  Area 2: **404-385-2000**  Area 3: **404-385-3000**  Area 4: **404-385-4000**  Area 5: **404-385-5000** |
| **GA Tech Pest Control** | **Facilities-Utilities & Energy** | <http://facilities.gatech.edu/pest-or-animal-control> |
| **Other Numbers** | | |
| **Insurance and Risk Management** | **Frederick Trotter** | **404-894-3483** |

In case of an emergency, call the Call the Georgia Tech Police Department at [404-894-2500](tel:404-894-2500) immediately if you are experiencing a life-threatening emergency or need a fire truck or ambulance.

For links to information about a campus-wide emergency, or to sign up for emergency alerts, go to [Georgia Tech's main emergency page](http://www.gatech.edu/emergency).

For emergency response for common incidents, visit <https://www.ehs.gatech.edu/emergency>

## POST INJURY/ILLNESS INSTRUCTIONS

**Faculty, Staff, & Employed Students:**

Injuries must be reported to the Shop Supervisor.

* If no medical attention is required, do not call DOAS 24-hour injury report line.
* If medical attention is required, the Supervisor must call DOAS 24-hour injury report line at (877) 656-7475.

Please Note:

* Agency Unit Location # - Georgia Tech: #7202
* You **DO NOT** have to give your Social Security Number (SSN)

**Georgia Tech Students that are not employed:**

The injury must be reported to the Shop Supervisor. In case of an injury, non-employed GA Tech students should visit Stamps Health Services.

Students requiring assistance after attention is sought for the injury/illness may contact the Georgia Tech student Affairs Office/Dean of Students

* During regular work hours call: 404-894-6367 (choose Option 9)
* After Hours/Weekends call GT Police: 404-894-2500 and ask them to page the Dean on Duty

**Supervisor must report injury to EHS:**

After the injury is reported to DOAS (if applicable) and/or Student Affairs (if applicable), the supervisor must report the injury to EHS.

* The supervisor must investigate the injury.
* The supervisor must fill out the “Supervisor Accident Investigation” Webform on the EHS website.
* Link to the Webform: <https://ehs.gatech.edu/content/supervisors-accident-investigation>

**For assistance contact:** [**generalsafety@ehs.gatech.edu**](mailto:generalsafety@ehs.gatech.edu)

## AUTHORIZATION FORM

**Student Name/GT ID#: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**(Print)**

**Shop Supervisor** **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**TO BE COMPLETED BY THE SHOP SUPERVISOR OF THE “AUTHORIZED USER”:**

Re: This document confirms the required qualification of the above-named employee to perform:

(Check all that apply)

□ **Operations and work in the following Shops:**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

□ **Operate and work with the shop equipment listed:**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

□ **Other Processes (describe):**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The qualification to work in the Maker Space and Student machine shop will be revoked if the user is not performing safely as trained. Below are signature(s) of responsible person(s) verifying training, experience and/or providing instruction.

**TO BE COMPLETED BY THE SHOP SUPERVISOR / SUPERVISOR:**

This designation of “Authorized User Form” is based on evidence of safe performance of all duties related to Maker Space and Student machine shop Safety and verification by the “Shop Supervisor / Supervisor” through:

*(Check all that apply)*

□ **Training:** Training Agreement Record and skills test attached.

□ **Experience:** Demonstrated skill in safe operation of Shop equipment for \_\_\_\_\_ years.

□ **Instruction**  This person has received instruction from me or another Maker Space and Student machine shop employee who is qualified/authorized and has observed this person’s work while performing Maker Space and Student machine shop operations and confirms that the person has the knowledge to perform Maker Space and Student machine shop work safely.

The authorized user agrees and understands that they are authorized to use only the equipment trained on that is noted above.

**Shop Supervisor/Supervisor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_**

**Authorized Person’s Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_**

## MAKER SPACE/ STUDENT MACHINE SHOP USER’S AGREEMENT

Professional Conduct is required

* Training is required to use any piece of equipment in the maker space/student machine shop space.
* Respect for others and school resources are required at all times.
* Horseplay is never appropriate in the maker space/student machine shop spaces.
* Be aware of others around your work, and the work being performed around you, at all times.
* Use the correct tool for the job and never abuse the tool. Use the training you have received.
* Avoid holding your work pieces with your hands when using cutting tools. Clamp your work piece in a vise and use two hands to hold the tool whenever possible.
* Know your physical limits. Do not operate power tools when you are too tired to be alert.
* Always report any injury, broken tool, housekeeping issue, or potential hazard.

Dress for the work being performed

* Personal protection equipment (safety glasses, ear plugs, breathing masks, etc.) are to be worn anywhere signs are posted in the workspace, or whenever appropriate based on good training for that tool. For example, safety glasses are to be worn anytime powered, sharp, or impact tools are being used in your vicinity.
* Never approach rotating or any large power tools with loose clothing, long untied hair, lanyards, headphone cords around your neck, or large jewelry that could pull you toward the machine.
* Shoes worn in the fabrication spaces must cover the tops of your feet.

Never Work Alone with Powered Tools

* You must have at least one work partner within at least voice distance of you whenever powered cutting tools are in operation. Visual distance is required for certain equipment as posted.
* You must not be separated by a closed door from this partner. Most certainly not a locked door.
* Your work partner must be trained (and able) to turn off the tool in the event of an emergency.
* Partner must be able to call the campus police (404) 894-2500 in any emergency.
* It is the user’s responsibility to confirm the above any time powered tools are in operation.

You Must Help Keep the maker space/student machine shops Safe as You Use Them

* You must clean your work area of any debris that you have created, or others have created before you. The next person using the space must find it to be clean, organized, and safe.
* You must help keep the floor space in the maker space/student machine shops dry and free of tripping or slipping hazards such as saw dust, oil, electrical cords, or raw materials.
* Whenever you use a tool, you are responsible for returning it to its proper storage location, regardless of where you found it. If you are unsure, please ask the lab personnel.
* Exits, corridors, and passageways must be kept clear of furniture or project prototypes for safe passage during an emergency.
* Never modify any tool, and especially, never remove safety devices from tools.
* If you see someone working in an unsafe manner, you must gently correct them as a colleague.
* Have Fun, keep learning, and teach others what you have learned!

The student agrees to the user’s agreement and also understands that they are authorized to use only the equipment in which they have received training on.

Sign and date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## HAZARD ASSESSMENT TOOL – PPE SELECTION

This document can be used as a supplement to the Hazard Assessment Tool in the selection of appropriate personal protective equipment (PPE) for the Maker Spaces and Student machine shops.

|  |  |  |  |
| --- | --- | --- | --- |
| **Applicable PPE** | **Specific type (example)** | **Characteristics** | **Applications** |
| **Light latex, vinyl, or nitrile gloves** | **Disposable latex gloves** | Powdered or un-powdered | Working with biological hazards (human blood, body fluids, blood borne pathogens, specimens) |
| **Disposable nitrile gloves** | Puncture, abrasion resistant, protection from splash hazards | Working with Biological Hazards and chemical splash hazards |
| **Disposable vinyl gloves** | Economical, durable, similar to latex | Biological Hazards |
| **Applicable PPE** | **Specific type (example)** | **Characteristics** | **Applications** |
| **Light chemical resistant gloves** | **Natural rubber latex** | Chemical resistant, liquid-proof | Working with small volumes of corrosive liquids, organic solvents, flammable compounds |
| **Light to heavy chemical resistant gloves** | **Nitrile gloves** | Chemical resistant, good puncture, cut, and abrasion resistance | Apparatus under pressure, air, or water reactive chemicals |
|  |  |  |  |
|  |  |  |  |
| **Heavy chemical resistant gloves** | **Butyl gloves** | High permeation resistance to most chemicals | Large volumes of organic solvents, small to large volumes of dangerous solvents, acutely toxic or hazardous materials |
| **Viton® II gloves** | High permeation resistance to most chemicals | Same as butyl gloves, plus hazardous material spills |
| **Insulated gloves** | **Terrycloth autoclave gloves** | Heat resistant | Working with hot liquids and equipment, open flames, oil bath |
| **Applicable PPE** | **Specific type (example)** | **Characteristics** | **Applications** |
|  | **Cryogen gloves** | Water resistant or waterproof, protection against ultra-cold temperatures | Cryogenic liquids handling |
| **Wire mesh gloves** |  | Cut resistant | Working with sharp tools or equipment |
|  |  |  |  |
|  |  |  |  |
| **Chemical resistant apron** | **Rubber-coated wash apron** | Chemical splash protection, good abrasion resistance | Working with apparatus under pressure, air or water reactive chemicals, large volumes of corrosive liquids |
| **Neoprene apron and sleeves** | Chemical resistant, tear resistant | Water or air reactive chemicals, large volumes of corrosive liquids, small to large volumes of acutely toxic corrosives |
| **Applicable PPE** | **Specific type (example)** | **Characteristics** | **Applications** |
| **Shop Aprons** | **Leather Shop Apron** | Protects clothing from dirt, dyes, debris, or non-hazardous chemicals | General industrial, maintenance, construction, carpentry, or shop applications |
| **Denim Shop Apron** | Protects clothing from dirt, dyes, debris, or non-hazardous chemicals | General industrial, maintenance, construction, carpentry, or shop applications |
| **Safety glasses** | **Glasses** | Polycarbonate lens, side shields for eye protection. Meets ANSI and OSHA specifications | Working with chemical, biological, or physical hazards. |
| **Safety glasses** | **Glasses/Goggle Hybrid** | Impact resistant lens with anti-fog coating and polyurethane foam seal | Working with chemicals, biological, dusty, or overhead work |
| **Laser Goggles** | Appropriately shaded goggles; optical density based on beam parameters | Working with Class 3 or Class 4 lasers |
| **Face shield** |  | Chemical resistant face shield | For use with mild acids, caustics, aromatic hydrocarbons. For use when splash hazard. For use when using air or water reactive or in operations that produce flying particles. |
| **Safety shield** |  | High-impact-resistant, clear polycarbonate, magnetic base. | Protects operators from flying chips (swarf), sparks, and splashing coolant generated at the machines point of operation |
| **Applicable PPE** | **Specific type (example)** | **Characteristics** | **Applications** |
| **Respirators**  **Must be a part of EHS Respiratory Protection Program.**  **Respirators** | **N-95** | Protects against dust, fumes, mists, microorganisms | Working with high amounts of debris or dusty environments. |
| **Half face** | Air purifying respirator protects against variety of particulates, vapors, dust, mists, fumes; depends on filter cartridge used | Working with high amounts of debris or dusty environments; chemical vapors; particulates |
| **Full face** | Same as half- face, but with greater protection factor, and greater protection of eyes and face; depends on filter cartridge used | Working with high amounts of debris or dusty environments; chemical vapors; particulates |
| **SCBA** | Self-Contained Breathing Apparatus is a device that provides air in an immediately dangerous to life and health (IDLH) atmosphere | Working in a confined space where the atmosphere is unpredictable or uncontrollable. |
| **Hearing Protection** | **Disposable Ear Plugs** | Polyvinyl Chloride (PVC) or Polyurethane foam, one time use design (no cleaning), one size fits all, light weight, low cost, blocks all sound | Working with high powered equipment such as shop machinery, power tools, or gas-powered equipment. |
| **Reusable Ear Plugs** | Silicone, tapered fit, reusable (needs cleaning), corded or uncorded, light weight, more durable than disposable | Working with high powered equipment such as shop machinery, power tools, or gas-powered equipment. Can be used for |
| **Hearing Band** | Ear plugs connected to a flexible band that can be worn around the neck when not needed | Working with high powered equipment such as shop machinery, power tools, or gas-powered equipment. |
| **Earmuffs** | One size fit all, fits better for longer periods of time, higher noise reduction rating, durable, dielectric | Working with high powered equipment such as shop machinery, power tools, or gas-powered equipment. |
| **Footwear Protection**  **Footwear Protection** | **Slip Resistant** | Slip resistant sole, comfortable, light weight | Working in areas with slip hazards (i.e., wet floors). Working in areas made of tile, marble, or terrazzo. |
| **Safety Boots** | Steel toe offers toe protection, durable, puncture resistant | Working in areas with power tools or heavy machinery used in construction. |
| **Chemical Resistant Boot** | High permeation resistance to most chemicals | Working with large amounts of chemical compounds or during chemical spill clean-up |

## MAKER SPACE AND STUDENT MACHINE SHOP SELF-INSPECTION FORM

|  |  |  |
| --- | --- | --- |
| **Shop Name:** |  | **Dept. Head:** |
| **Building Name:** |  | **Supervisor:** |
| **Department:** |  | **RTK Coord:** |
| **Room No:** |  | **Laser Supervisor:** |
| **Building Manger:** | **Inspection Date:** | **Inspector:** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Power Platforms, Manlifts, Vehicle-Mounted Platforms** | **Yes** | **No** | **N/A** |
| 1. Employees standing on floor of the basket, not on any other devices for work position. |  |  |  |
| 1. Building anchors visible, stabilizer tie at platform suspension ropes at each vertical interval. |  |  |  |
| 1. Man lift and driving mechanisms protected from weather at all times. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Fall Protection** | **Yes** | **No** | **N/A** |
| 1. Locking type with a self-closing, self-locking keeper remains closed. |  |  |  |
| 1. Personal fall arrest system used by workers on surfaces more than 4 feet. |  |  |  |
| 1. Body harnesses inspected before use each day. |  |  |  |
| 1. Rails used with at least 42” high mid-rails and toe boards. |  |  |  |
| 1. Portable ladders in good condition. Ladder rungs and steps uniformly spaced. |  |  |  |
| 1. Extension ladders have stabilizers and leg levelers. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Lockout/Tagout** | **Yes** | **No** | **N/A** |
| 1. Employees following procedures of a written lockout/tagout plan. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Machine Guarding** | **Yes** | **No** | **N/A** |
| 1. The point of operation of machinery that may cause injury is guarded. |  |  |  |
| 1. Each machine free from sensible vibration when idled at full speed. |  |  |  |
| 1. All trip and emergency switches require manual setting. |  |  |  |
| 1. Grinder wheel in good condition. |  |  |  |
| 1. Work rests adjusted closely to the wheel with a maximum opening of 1/8 inch. |  |  |  |
| 1. Machine components covered to reduce release of mechanical energy. |  |  |  |
| 1. Expanded metal, sheet, or wire mesh securely fastened to frame. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Electrical Safety** | **Yes** | **No** | **N/A** |
| 1. Are there > 3 ft. of working space in front of switchboards or motor control center’s? |  |  |  |
| 1. Electrode and circuit conductors attached to grounding electrode. |  |  |  |
| 1. Branch circuits originate in a power outlet or panel board. |  |  |  |
| 1. Single mean to disconnect ungrounded main power supply conductors. |  |  |  |
| 1. Equipment provided protection from combustible and flammable hazards. |  |  |  |
| 1. Conductors emerging from the ground in enclosed raceways. |  |  |  |
| 1. GFCIs used on electrical equipment where there is moisture or wetness. |  |  |  |
| 1. Extension cords are used for temporary work only. |  |  |  |
| 1. All junction boxes are covered (no exposed wiring). |  |  |  |
| 1. All wall outlets are covered. |  |  |  |
| 1. All light switches are covered. |  |  |  |
| 1. Any light that is at risk of being struck is properly covered. |  |  |  |
| 1. Power strips are not overloaded. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Fire** | **Yes** | **No** | **N/A** |
| 1. Fire extinguishers are accessible with less than 75 feet of travel to any extinguisher. |  |  |  |
| 1. Fire extinguishers are inspected annually and tagged (current inspection). |  |  |  |
| 1. Flammable aerosols and liquids are stored properly (flammables cabinet). |  |  |  |
| 1. There is sufficient clearance (18”) between the top of storage and sprinkler heads For ESFR heads, clearance is 36”. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Tool Safety** | **Yes** | **No** | **N/A** |
| 1. All hand and power tools equipped with guards where applicable. |  |  |  |
| 1. Tools free from structural defects and in good condition. |  |  |  |
| 1. Safety clips attached to prevent attachments from being expelled. |  |  |  |
| 1. When pressure released, pressure switch or control shuts off power. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Compressed Gas Cylinders** | **Yes** | **No** | **N/A** |
| 1. Portable tanks and cargo tanks have pressure relief devices. |  |  |  |
| 1. Legibly marked with the name of the gas. |  |  |  |
| 1. Secured individually in upright position. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Personal Protective Equipment (PPE)** | **Yes** | **No** | **N/A** |
| 1. PPE appropriate for hazards. Employees are certified on proper use, care, and storage of PPE. |  |  |  |
| 1. Eye and face protection available. |  |  |  |
| 1. Provide adequate protection against hazards for which they are designed. |  |  |  |
| 1. Protective helmet when working in areas where there is potential for falling objects. |  |  |  |
| 1. Protective footwear when working in areas where there is danger of foot injuries. |  |  |  |
| 1. Hand protection against skin abrasions, punctures, chemical burns, and temperature extremes. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Hazardous Materials** | **Yes** | **No** | **N/A** |
| 1. All containers properly labelled. |  |  |  |
| 1. Safety Data Sheets (SDS) kept up to date and available to employees. |  |  |  |
| 1. Hazardous materials are stored properly. |  |  |  |
| 1. Are chemicals added to EHSA (campus inventory database)? |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Walking/Working Surfaces** | **Yes** | **No** | **N/A** |
| 1. Areas clean and orderly. Aisles and passageways clear and in good repair. |  |  |  |
| 1. Barriers around opening – drop of 4’. Rail, toe board around exposed side of opening. |  |  |  |
| 1. Clearance between machines – movement of one operator does not interfere with others. |  |  |  |
| 1. Working spaces, walkways, and similar locations clear of cords. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **General Safety and Health Provisions** | **Yes** | **No** | **N/A** |
| 1. Employees aware of procedures for reporting injuries. |  |  |  |
| 1. Suitable facility for washing, flushing eyes, or body shower. |  |  |  |

**Additional Items:**